

**Exhibit B 2– Performance Requirements- Category 2 Pressure Washing**

|  |  |
| --- | --- |
| Competitive Solicitation: | No. 25423- Graffiti Removal Services |
| Bidder: | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Type/print full legal name of bidder company |

**Instructions**

1. Add bidder company’s name above and review the below Performance Requirements.
2. Mark YES or NO if bidder meets each requirement in **Bidder’s Compliance** column.
3. Submit the exhibit as a Microsoft Word document and without modifying the font or formatting. If you need to print out this document for any reason, please note this document is size Legal 8.5” x 14”.

*Please note*: Not following any of the specified instructions might be grounds for the bid to be considered non-responsive.

| **Performance Requirements and Factors** |
| --- |
| **Requirement ID** | **Performance Requirement and****Stated Business Need** | **Bidder’s Compliance** |
| 1. | The Contractor shall implement the best processes for the prevention of stormwater pollution in conjunction with all its activities and operations:WASTE MANAGEMENTSolid Waste ManagementHazardous Waste ManagementSanitary/Septic Waste Management | [ ]  Yes[ ]  No |
| 2. | Stormwater or dewatering water that has come in contact with concrete rubble, concrete pours, or cement-treated soils shall be maintained to pH 8.5 or less before it is allowed to enter the waters of the State or the City stormwater system. High pH process water shall not be discharged to the State or the City stormwater system waters. | [ ]  Yes[ ]  No |
| 3. | Bidder shall prepare and implement a project-specific Construction Stormwater Pollution Prevention Plan (SWPPP)[Construction stormwater permit - Washington State Department of Ecology](https://ecology.wa.gov/regulations-permits/permits-certifications/stormwater-general-permits/construction-stormwater-permit) | [ ]  Yes[ ]  No |
| 4. | The range of pressure washing shall consist of horizontal and vertical washing and shall include but not be limited to bridges, sidewalks, walls, concrete, exterior masonry, etc. Pressure washing shall remove all foreign material from the exterior finish. The Contractor will provide all apparatus for safe operation at heights, including ladders, scaffolds, man-lifts, etc. | [ ]  Yes[ ]  No |
| 5 | The Contractor shall perform all work in accordance with the manufacturer’s recommended cleaning procedures for the specific surface being washed, applicable codes, local ordinances, and requirements.  | [ ]  Yes[ ]  No |
| 6 | The Contractor shall have technical knowledge to support the correct application of pressure and any chemicals used in the pressure washing process. Care is to be taken to ensure there is no damage to the exterior and/or interior surfaces being washed. Products used shall be green seal certified or equivalent. | [ ]  Yes[ ]  No |
| 7 | The contractor Shall use a Hot water pressure washing rig with a self-contained water tank and the capacity to vacuum up wastewater “Necessary to prevent runoff into storm drains.” | [ ]  Yes[ ]  No |
| 8 | Bidder has policies and procedures to prevent polluted pressure-washing wastewater from entering the storm system. For example, the bidder places a filter over or creates a barrier around storm drains. | [ ]  Yes[ ]  No |

Return this exhibit to Procurement Coordinator at:
DESContractsTeamMaple@des.wa.gov